DEPARTMENT OF PUBLIC HEALTH AND ENVIRONMENT

Solid and Hazardous Waste Commission/Hazardous Materials and Waste Management Division

6 CCR 1007-3

hazardous waste

Amendment of § 261.21 Characteristic of ignitability.

(Adopted by the Solid and Hazardous Waste Commission on May 19, 2015)

1) Revise § 261.21 to read as follows:  

§ 261.21 Characteristic of ignitability.

(a) A solid waste exhibits the characteristic of ignitability if a representative sample of the waste has any of the following properties: 

(1) ******* 

(2) *******
 
(3) It is an ignitable compressed gas. 

(i) The term “compressed gas” shall designate any material or mixture having in the container an absolute pressure exceeding 40 p.s.i. at 70ºF or, regardless of the pressure at 70ºF, having an absolute pressure exceeding 104 p.s.i. at 130ºF; or any liquid flammable material having a vapor pressure exceeding 40 p.s.i. absolute at 100ºF as determined by ASTM Test D-323.

(ii) A compressed gas shall be characterized as ignitable if any one of the following occurs:
 
(A) Either a mixture of 13 percent or less (by volume) with air forms a flammable mixture or the flammable range with air is wider than 12 percent regardless of the lower limit. These limits shall be determined at atmospheric temperature and pressure. The method of sampling and test procedure shall be acceptable to the Bureau of Explosives and approved by the director, Pipeline and Hazardous Materials Technology, U.S. Department of Transportation (see Note 2).

(B) Using the Bureau of Explosives' Flame Projection Apparatus (see Note 1), the flame projects more than 18 inches beyond the ignition source with valve opened fully, or, the flame flashes back and burns at the valve with any degree of valve opening.

(C) Using the Bureau of Explosives' Open Drum Apparatus (see Note 1), there is any significant propagation of flame away from the ignition source.

(D) Using the Bureau of Explosives' Closed Drum Apparatus (see Note 1), there is any explosion of the vapor-air mixture in the drum.

(4) It is an oxidizer.  An oxidizer for the purpose of this subchapter is a substance such as a chlorate, permanganate, inorganic peroxide, or a nitrate, that yields oxygen readily to stimulate the combustion of organic matter (see Note 4).

(i) An organic compound containing the bivalent -O-O- structure and which may be considered a derivative of hydrogen peroxide where one or more of the hydrogen atoms have been replaced by organic radicals must be classed as an organic peroxide unless:

(A) The material meets the definition of a Class A explosive or a Class B explosive, as defined in § 261.23(a)(8), in which case it must be classed as an explosive,

(B) The material is forbidden to be offered for transportation according to 49 CFR 172.101 and 49 CFR 173.21,

(C) It is determined that the predominant hazard of the material containing an organic peroxide is other than that of an organic peroxide, or

(D) According to data on file with the Pipeline and Hazardous Materials Safety Administration in the U.S. Department of Transportation (see Note 3), it has been determined that the material does not present a hazard in transportation.

(b) A solid waste that exhibits the characteristic of ignitability has the EPA Hazardous Waste Number of D001.

Note 1: A description of the Bureau of Explosives' Flame Projection Apparatus, Open Drum Apparatus, Closed Drum Apparatus, and method of tests may be procured from the Bureau of Explosives.

Note 2: As part of a U.S. Department of Transportation (DOT) reorganization, the Office of Hazardous Materials Technology (OHMT), which was the office listed in the 1980 publication of 49 CFR 173.300 for the purposes of approving sampling and test procedures for a flammable gas, ceased operations on February 20, 2005. OHMT programs have moved to the Pipeline and Hazardous Materials Safety Administration (PHMSA) in the DOT.

Note 3: As part of a  U.S. Department of Transportation (DOT) reorganization, the Research and Special Programs Administration (RSPA), which was the office listed in the 1980 publication of 49 CFR 173.151a for the purposes of determining that a material does not present a hazard in transport, ceased operations on February 20, 2005. RSPA programs have moved to the Pipeline and Hazardous Materials Safety Administration (PHMSA) in the DOT.

Note 4: The DOT regulatory definition of an oxidizer was contained in § 173.151 of 49 CFR, and the definition of an organic peroxide was contained in paragraph 173.151a. An organic peroxide is a type of oxidizer.

2) Add Section 8.84 {Statement of Basis and Purpose for the Rulemaking Hearing of May 19, 2015} to Part 8 of the Regulations to read as follows:

Statement of Basis and Purpose
Rulemaking Hearing of May 19, 2015

8.84	Basis and Purpose.

This amendment to 6 CCR 1007-3, Part 261 is made pursuant to the authority granted to the Solid and Hazardous Waste Commission in § 25-15-302(2), C.R.S.

Amendment of § 261.21 Characteristic of ignitability.

These amendments to § 261.21 of the Colorado Hazardous Waste Regulations (6 CCR 1007-3) replace the obsolete references to the DOT regulations contained in the definitions for an ignitable compressed gas (§ 261.21(a)(3)) and an oxidizer (§ 261.21(a)(4)), with the actual language from the referenced sections of the DOT regulations that was published in Title 49 of the CFR at the time of the finalization of the RCRA regulations (1980). Because it can be difficult to obtain copies of the CFR from 1980, these amendments will make it easier for the regulated community to find and apply the definitions of ignitable compressed gas and oxidizer for the purposes of § 261.21. The implementation and enforcement of the ignitability characteristic will not change in any way. The Division is simply publishing the original definitions to ease the burden on the regulated community.

This Basis and Purpose incorporates by reference the applicable portions of the preamble language for Section 261.21 of the EPA regulations as published in the Federal Register at 71 FR 40254-40255, July 14, 2006.