BASIS AND PURPOSE FOR AMENDMENTS TO RULE 12
The purpose of Rule 12 is to establish specifications for $10 and $25 tokens. The statutory basis for Rule 12 is found in sections 12-47.1-201, C.R.S., 12-47.1-203, C.R.S., and 12-47.1-302, C.R.S.
RULE 12  GAMING DEVICES AND EQUIPMENT
47.1-1216  Specifications for tokens.
(1)    	One-dollar metal tokens must be disk-shaped and must measure from 1.459 through 1.474 inches in diameter, from .095 through .115 inch thick.   Eff  03/02/2007
(2)  	Two dollar metal tokens must be disk-shaped and must measure from 1.292 inches through 1.392 inches in diameter, from .092 inches through .104 inches thick.   Eff  03/02/2007
(3)  	Five dollar metal tokens must be disk-shaped and must measure from 1.740 inches through 1.760 inches in diameter, from .115 inches through .135 inches thick.   Eff  03/02/2007
(4)	Ten dollar metal tokens must be disk-shaped and must measure from 1.700 inches through 1.760 inches in diameter, from .096 inches through .104 inches thick.
(5)	Twenty-five dollar metal tokens must be disk-shaped and must measure from 1.650 inches through 1.710 inches in diameter, from .096 inches through .104 inches thick.
(4)(6)  	Metal tokens must not be manufactured from material possessing sufficient magnetic properties to allow it to be accepted by a coin mechanism other than that of a slot machine. Metal tokens may not be manufactured from a three-layered material consisting of a copper-nickel alloy clad on both sides of a pure copper core nor from a copper-based material unless the total of zinc, nickel, aluminum, magnesium, and other alloying materials is at least 20 percent of the token’s weight.   Eff  03/02/2007